**FINAL CHECKLIST FOR COORDINATION OF ROADWAY AND STRUCTURE PLANS**

**TIP NO:** **COUNTY:**

1. Beginning and ending stations shown on Roadway Plans for bridge agree with Structure Plans.

2. Pay items on Structure Plans agree with the pay items on the Roadway Plans (Example – If rip-rap is required, do not show the rip-rap on Structure Plans and dumped stone on Roadway Plans).

3. Guardrail attachments on structure and roadway plans are attached at the same points and located on the same corners.

4. Bridge widths on Roadway Plans (if shown) agree with widths on Structure Plans.

5. Shoulder to shoulder widths beneath the bridge on a grade separation shown on the Structure Plans agree with widths shown on the typical sections in the Roadway Plans.

6. Drainage Structures shown on the structure plans agree with Drainage Structures shown on Roadway Plans.

7. Note shown stating that existing pavement shall be scarified in area of end-bent piles.

8. Pay Items and Roadway Standard Drawings or details are included in the Roadway Plans for (check one):

\_\_\_Type I Standard Approach Fill.

\_\_\_Type II Modified Approach Fill.

\_\_\_Type III Reinforced Approach Fill.

9. Vertical and Horizontal Alignment on Roadway Plans agree with that shown on Structure Plans.

Checked By (Rdy): Date:

Checked By (Str): Date: