**FINAL CHECKLIST FOR COORDINATION OF ROADWAY AND STRUCTURE PLANS**

**TIP NO:** **COUNTY:**

1.[ ]  Beginning and ending stations shown on Roadway Plans for bridge agree with Structure Plans.

2.[ ]  Pay items on Structure Plans agree with the pay items on the Roadway Plans (Example – If rip-rap is required, do not show the rip-rap on Structure Plans and dumped stone on Roadway Plans).

3.[ ]  Guardrail attachments on structure and roadway plans are attached at the same points and located on the same corners.

4.[ ]  Bridge widths on Roadway Plans (if shown) agree with widths on Structure Plans.

5.[ ]  Shoulder to shoulder widths beneath the bridge on a grade separation shown on the Structure Plans agree with widths shown on the typical sections in the Roadway Plans.

6.[ ]  Drainage Structures shown on the structure plans agree with Drainage Structures shown on Roadway Plans.

7.[ ]  Note shown stating that existing pavement shall be scarified in area of end-bent piles.

8.[ ]  Pay Items and Roadway Standard Drawings or details are included in the Roadway Plans for (check one):

\_\_\_Type I Standard Approach Fill.

\_\_\_Type II Modified Approach Fill.

\_\_\_Type III Reinforced Approach Fill.

9.[ ]  Vertical and Horizontal Alignment on Roadway Plans agree with that shown on Structure Plans.

Checked By (Rdy): Date:

Checked By (Str): Date: