**REMOVE AND REPLACE SNOWPLOWABLE PAVEMENT MARKER REFLECTOR:**

|  |  |
| --- | --- |
| (02/06/2013) |  |

Page 12-16, Article 1253-3(B) Reflector Replacement, add the following after the first paragraph:

Remove existing Snowplowable Pavement Marker Reflective Lenses as specified in the plans by the method recommended by the manufacturer of the marker and approved by the Engineer.

Install new Reflective Lenses in existing Snowplowable Pavement Marker Castings as specified in the plans by using adhesives and methods recommended by the manufacturer of the markers and approved by the Engineer.

Missing castings shall be replaced. Broken castings shall be removed and replaced. In both cases, the slot for the castings shall be properly prepared by the method recommended by the manufacturer of the marker prior to installing the new casting. Removal of broken castings and preparation of slots will be considered incidental to the work of replacing castings.

Page 12-16, Article 1253-5 Measurement and Payment, add the following as the second paragraph:

*Remove and Replace Snowplowable Pavement Marker Reflector* will be measured and paid for in units of each that have been satisfactorily removed, replaced and accepted.

Add the following pay item:

|  |  |
| --- | --- |
| Pay Item | **Pay Unit** |
| Remove and Replace Snowplowable Pavement Marker Reflector | Each |