**PROTECTIVE CANOPY:**

(06/28/2013)

**Description**

The Contractor shall provide a protective canopy to protect pedestrians from falling debris along the existing sidewalk beneath the \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ bridge structure at all times during construction.

**Construction Methods**

The protective canopy shall be constructed in accordance with local governing building codes, and requirements of the Americans with Disabilities Act (ADA). The protective canopy shall be adequately lit for nighttime use. At no time shall materials or equipment be stored on the canopy roof. All waste or falling debris is to be removed from the canopy roof on a daily basis or as directed by the engineer. The Contractor is to investigate and secure all necessary permits required by the governing bodies aforementioned prior to commencing work.

**Measurement and Payment**

The measurement and payment for the Protective Canopy shall be Lump Sum. The Lump Sum price shall include any costs associated with the installation, maintenance and removal.

**Pay Item Pay Unit**

Protective Canopy Lump Sum