                      North Carolina Department of Transportation                                        NCDOT M&T Form 250VM


                 AGGREGATE MOISTURE REPORT
                        FOR VOLUMETRIC CONCRETE MOBILE MIXER 
 
     Date of   Calibration                                                      Project Number            	                                              
      Fine Aggregate Source                	          	          	          	          	                      
      Coarse Aggregate Source                   	          	          	          	          	                                                          

	Class of Concrete
	Mix Design No.
	Number of Loads
	Total Yards Batched

	     
	     
	     
	     

	     
	     
	     
	     



                      MOISTURE IN AGGREGATES

     Fine Aggregate:	
[bookmark: _Hlk134688500]                                                                                           Trial 1                                               Time: _     _
                                                                                                                                                           
[bookmark: _Hlk134687601][bookmark: _Hlk132178339][bookmark: _Hlk134688298]               Wet Wt. _     _     Minus             Dry Wt. _     _
· -------------------------------------------------------------------------------------------------------------------------------------------------------------------------                      =    _     _     X     100  =  _     _ % Total Moisture
                                        Dry Wt. _     _
                                     …………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………..………………..
· Total  Moisture _     _     Minus         Absorbed Moisture _     _   =    _     _ % Free Moisture
                                                                                      
                                                                                       Trial 2                                               Time: _     _
                                                                                                    
               Wet Wt. _     _     Minus             Dry Wt. _     _
· -------------------------------------------------------------------------------------------------------------------------------------------------------------------------                      =   _     _      X      100  =    _     _ % Total Moisture
                                        Dry Wt. _     _
…                                                          ……………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………....
· Total   Moisture _     _       Minus          Absorbed Moisture _     _  =     _     _ % Free Moisture

     Coarse Aggregate:                                     
                                                                                       Trial 1                                               Time: _     _                                       

               Wet Wt. _     _    Minus           Dry Wt. _     _
· -------------------------------------------------------------------------------------------------------------------------------------------------------------------------                      =   _     _          X  100    =    _     _ % Total Moisture
                                        Dry Wt. _     _
                                            ……………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………
· Total  Moisture _     _     Minus        Absorbed Moisture _     _     =     _     _ % Free Moisture
                                                                                      
                                                                                       Trial 2                                               Time: _     _
                                                                                                    
               Wet Wt. _     _     Minus           Dry Wt. _     _
· -------------------------------------------------------------------------------------------------------------------------------------------------------------------------                      =   _     _          X   100    =   _     _ % Total Moisture
                                        Dry Wt. _     _
                                                 ………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………..
· Total  Moisture _     _     Minus        Absorbed Moisture _     _     =     _     _ % Free Moisture


                
[bookmark: _Hlk151112994]                                                           Certified Technician:                 	          Certification No.              

North Carolina Department of Transportation
Field Calibration Report for
 Latex Modified Concrete Mobile Continuous Mixer



Mixer Number:       	 Calibrated By:       	
Project: _     ____________________

Date of Calibration:       	 Mix Design:       		
Resident Engineer: _     _________

Step 1 - Cement Output 

[bookmark: _Hlk142394365]        C.  Use a stopwatch to determine the time and meter counts required to discharge a minimum 
              of  100 pounds of cement into a container. 

                     Record all weights and meter counts to the nearest tenth. Record time to the nearest hundredth of a second.
            **Notes:   -        Aggregate bins must be empty during cement calibration to prevent sand and/or any stone particles from
                                              being conveyed with the cement. 
·  The tolerance on cement weight is 0% to plus 4% (i.e., 100 – 104 lb). A value slightly above 104 lb may be
           considered reasonably close. 

         D.   A minimum of 5 of these determinations (runs) shall be conducted.
	
	Run 1
	Run 2
	Run 3
	Run 4
	Run 5
	
	   E.    Total

	Cement Weight
 in pounds
	
     
	
     
	
     
	
     
	
     
	
     
	
     

	Meter Counts
	
     
	
     
	
     
	
     
	
     
	
     
	
     

	Time in Seconds
	
     
	
     
	
     
	
     
	
     
	
     
	
     



F. Determine the Cement Output per one Meter Count:

      	÷        	=         	lbs.
Total Cement Weight	Total Meter Counts	Cement Output per count

G. Determine the number of Meter Counts per 1 yd³ of concrete:

      	 ÷       	=        	
Total Design Cement Weight	Cement Output per count	Counts per 1 yd³

H. Determine the Time to produce 1 yd³ of concrete:

      	 ÷        	X        	=       	sec.
Total Time	Total Cement Weight	Total Design Cement Weight	Time per 1 yd³


                  **Note: The calculated result “Time to produce 1 yd³ of concrete” will be used in the Fine Aggregate (Sand) Gate    Calibration, 
                                  Coarse Aggregate ( Stone) Gate Calibration, Latex Flow Calibration and Water Flow Calibration calculations.

Rev. Sep. 2026

Step 2 – Fine Aggregate (Sand) Gate Calibration

A. Determine the amount of free moisture on the surface of the fine aggregate.

B. Determine the weight of wet fine aggregate (sand) to be batched for 1 yd3 of concrete:
      	 X        	=       	+       	=       	lbs.
SSD Design Sand Weight	Free Sand Moisture	SSD Design Sand Weight	Wet Sand Weight

C. Determine the weight of wet fine aggregate (sand) to be batched for 1/12 yd3 of concrete:
                      
                    **Note: 1/12 part of the mix will be considered optimal weight of aggregates for the calibration process only.

        	÷ 	12	=             	lbs.
Wet Sand Weight	Wet Sand Weight per 1/12 part of the Mix

[bookmark: _Hlk142394902]                                                                               (With tolerance ±2%:             to                lbs.)


D. Determine the time to produce 1/12 yd3 of concrete:

        	    _÷   	12	=         	sec.
  Time per 1 yd³ mix                                                           Time to produce 1/12 part of the Mix
 (Calculation in Step 1h) 	                                                       

E. Adjust the gate settings to discharge the target amount of fine aggregate (sand), within ± 2%, 
in the  same amount of time required to discharge 1/12 of the target cement weight per 1 yd3:

                                  **Note: The allowable aggregate weight tolerance is ± 2%.

(The gate setting needs to be adjusted to discharge         pounds of sand ±2%, within          seconds)

	
	Run 1
	Run 2
	Run 3
	Run 4
	Run 5
	

	Gate Setting
	
     
	
     
	
     
	
     
	
     
	
     

	Time
in seconds
	
     
	
     
	
     
	
     
	
     
	
     

	Sand Weight
in pounds
	
     
	
     
	
     
	
     
	
     
	
     



F. It is recommended that 5 determinations (runs) of Fine Aggregate (Sand) be conducted. Additional determinations may be conducted as needed to verify consistency. 





                   Fine Aggregate (Sand) Gate Setting:       	

Step 3 – Coarse Aggregate (Stone) Gate Calibration

A. Determine the amount of free moisture on the surface of the coarse aggregate.

B. Determine the weight of wet coarse aggregate (stone) to be batched for 1 yd³ of concrete:

         	X          	=          +        	    =               	lbs.
SSD Design Stone Weight	Free Stone Moisture	          SSD Design Stone Weight       Wet Stone Weight

C. Determine the weight of wet coarse aggregate (stone) to be batched for 1/12 yd3 of concrete:
        **Note: 1/12 part of the mix will be considered optimal weight of aggregates for the calibration process only.
   
           	÷	12	=                                              lbs.
Wet Stone Weight	   Wet Stone Weight per 1/12 part of the Mix

(With tolerance ±2%:       	to       	lbs.)

D. Determine the time to produce 1/12 yd3 of concrete:

            	÷	12	=                	__sec.
Time per 1 yd³ of mix	         Time to produce 1/12 part of the Mix
                                      (Calculation result from step 1h)


E. Adjust the gate settings to discharge the target amount of coarse aggregate (stone), within ± 2%,  
in the  same amount of time required to discharge 1/12 of the target cement weight per 1 yd3:
                         
                              **Note: The allowable aggregate weight tolerance is ± 2%.
(The gate setting needs to be adjusted to discharge         pounds of stone ±2%, within          seconds)

	
	Run 1
	Run 2
	Run 3
	Run 4
	Run 5
	

	Gate Setting
	
     
	
     
	
     
	
     
	
     
	
     

	Time
in seconds
	
     
	
     
	
     
	
     
	
     
	
     

	Stone Weight
in pounds
	
     
	
     
	
     
	
     
	
     
	
     



F. It is recommended that 5 determinations (runs) of Stone be conducted.
                    Additional determinations may be conducted as needed to verify consistency.



                    Coarse Aggregate (Stone) Gate Setting:       	

Step 4 – Latex Flow Calibration

A. Latex flow calibration can be determined by using the actual unit weight of latex emulsion  per gallon, or use the default value of the unit weight equals 8.5 lb./gal.

B. Determine the target weight of latex emulsion per 1/6 yd3 of the concrete mix:
                      
                           **Note: 1/6 part of the mix will be considered optimal weight (volume) of Latex for the calibration process only.

          gal.	÷ 	6	= ____     _____________ gal.
Total Latex Volume                                        Target Latex Volume for 1/6 part of the Mix


__       gal. __________ X   	8.5_lb./gal_ =	__     __________ lbs.
  Target Latex Volume for 1/6 part of the Mix 	      Unit weight of latex	Target weight of latex for 1/6 mix

(With tolerance ±3%:        to        lbs.)


C. Determine the time to produce 1/6 yd3 of concrete:

             	____ ÷   6     =                                      sec.
Time per One c. yd. of mix                                   Target Time for 1/6 part of the Mix
(Calculation result from step 1h)


D. [bookmark: _Hlk136511970]Adjust the Latex flow setting to discharge the target weight of Latex, within ± 3%, in the same amount of time required to discharge 1/6 of the target cement weight per 1 yd3.
      
        **Note: The allowable Latex Weight or Volume Tolerance is ±3%.

(The Latex flow setting needs to be adjusted to discharge           pounds of Latex ±3%, within         seconds)

	
	Run 1
	Run 2
	Run 3
	Run 4
	Run 5
	

	Latex Flow
      Setting
	
     
	
     
	
     
	
     
	
     
	
     

	Time
in seconds
	
     
	
     
	
     
	
     
	
     
	
     

	Latex Weight
in pounds
	
     
	
     
	
     
	
     
	
     
	
     




E. It is recommended that 5 determinations (runs) of Latex be conducted.                           Additional determinations may be conducted as needed to verify consistency.
                           





            Latex Flow Setting:       	

Step 5 - Water Flow Calibration

A. Determine the total weight of free water that is on the surface of the sand (FA) and  stone (CA) combined. Convert this weight to gallons by dividing by 8.33:

Sand:            	 X __     ___  _ =                           	 lbs.
 SSD Design Sand Weight	Free Sand Moisture	 Weight of Free Water in Sand

Stone:    _     ________ X                       =                	 lbs.
  SSD Design Stone Weight	Free Stone Moisture	   Weight of Free Water in Stone

              	 +                 	=       	÷ _8.33_=           	_ gal.
Weight of Free Water in Sand	   Weight of Free Water in Stone    	    Volume of Free Water


B. Determine the target weight of metered water required per 1 yd3 of concrete and per 1/6 yd3of concrete:

                                          gal.	 -            gal.	=           gal.          X _8.33_=          	lbs.
                                          Design Water Volume	   Volume of Free Water	   Target Water Volume	           Total Water Weight

                                  **Note: 1/6 part of the mix will be considered optimal weight (volume) of Water for the calibration process only.

            lbs.	÷	6	 =                    	lbs.
                                      Total Water Weight                                            Target Water Weight for 1/6 part of the Mix

[bookmark: _Hlk142462991](With tolerance ±1%:       	to        	lbs.)

C. Determine the time to produce 1/6 yd3 of concrete:

             	_____ ÷ 	6__ =                  	sec.
Time per 1 yd³ of mix	                      Target Time for 1/6 part of the Mix
(Calculation result from step 1h)
                    
                           
D. [bookmark: _Hlk136512039]Adjust the Water flow setting to discharge the target weight of Water, within ± 1%, in the same amount of time required to discharge 1/6 of the target cement weight per 1 yd3.
            
                    **Note: The allowable Water Weight or Volume Tolerance is ±1%.
(The Water flow setting needs to be adjusted to discharge           pounds of water ±1%, within        seconds)

	
	Run 1
	Run 2
	Run 3
	Run 4
	Run 5
	

	   Water Flow 
    Setting
	
     
	
     
	
     
	
     
	
     
	
     

	Time 
in seconds
	
     
	
     
	
     
	
     
	
     
	
     

	Water Weight
in pounds
	
     
	
     
	
     
	
     
	
     
	
     



E. It is recommended that 5 determinations (runs) of Water be conducted.                                Additional determinations may be conducted as needed to verify consistency.

            Water Flow Setting:       	

Field Calibration Summary

LMC Mobile Continuous Mixer #       		__ 
Concrete Producer:       	__________
Date of calibration:       	_____ 
Project:        		_____ 
Calibrated by:       			 ____________________________________________________________________________________________________________________________________________________
Mix Design:       				____ 
Moisture during calibration: FA         		%
CA        	%



	FINE AGGREGATE
GATE SETTING
	  
        

	COARSE AGGREGATE
GATE SETTING
	
 
                  

	LATEX EMULSION FLOW 
SETTING
	

                          

	WATER FLOW 
SETTING
	

                        

	METER COUNT PER
1 CUBIC YARD OF CONCRETE
	

                

	METER COUNTS PER ¼ YD³
(For Yield Test Purpose)
	

                 




