**PAVING INTERSECTIONS:**

|  |  |  |
| --- | --- | --- |
| (7-1-95) (Rev. 8-21-12) | 610 | SP6 R67AR |

Surface all unpaved intersections back from the edge of the pavement on the main line of the project at least 50 feet. The pavement placed in the intersection shall be of the same material and thickness placed on the main line of the project.

Resurface all paved intersections back to the ends of the radii, or as directed by the Engineer.

The base on the unpaved intersections will be placed and prepared for surfacing by State Forces.

Widen the pavement on curves as directed by the Engineer.