**SHOULDER WEDGE:**

|  |  |  |
| --- | --- | --- |
| (9-20-11) (Rev. 8-21-12) | 610 | SP6 R03R |

Revise the *2018* *Standard Specifications* as follows:

**Page 6-21, Article 610-8**, **SPREADING AND FINISHING**, add the following after line 39:

Attach a device, mounted on screed of paving equipment, capable of constructing a shoulder wedge with an angle of 30 degrees plus or minus 4degrees along the outside edge of the roadway, measured from the horizontal plane in place after final compaction on the final surface course. Use an approved mechanical device which will form the asphalt mixture to produce a wedge with uniform texture, shape and density while automatically adjusting to varying heights.

Payment for use of this device will be incidental to the other pay items in the contract.