**MILLING ASPHALT PAVEMENT:**

|  |  |  |
| --- | --- | --- |
| (1-15-19) | 607  | SP6 R59 |

Revise the *2018* *Standard Specifications* as follows:

**Page 6-5, Article 607-2, EQUIPMENT, lines 14-16,** delete the seventh sentence of this Article and replace with the following:

Use either a non-contacting laser or sonar type ski system with a minimum of three referencing stations mounted on the milling machine at a length of at least 24 feet.