**ADJUSTMENT OF OVERSIZED MANHOLES:**

|  |  |  |
| --- | --- | --- |
| (11-15-22) | 858 | SP8 R94R |

Revise the *2018* *Standard Specifications* as follows:

**Page 8-38, Article 858-4 MEASUREMENT AND PAYMENT,** add the following paragraph after line 9:

*Adjustment of Oversized Manholes* will be measured and paid in units of each for oversized manholes satisfactorily adjusted and accepted by the Engineer.

**Page 8-38, Article 858-4 MEASUREMENT AND PAYMENT,** add the following paragraph after line 17:

Manholes with a frame and cover top diameter greater than 30 inches and/or frame height greater than 12 inches shall be measured and paid as *Adjustment of Oversized Manholes*.

**Page 8-38, Article 858-4 MEASUREMENT AND PAYMENT,** add the following after line 22:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| Adjustment of Oversized Manholes | Each |