**ADJUSTMENT OF CATCH BASINS, MANHOLES, DROP INLETS, METER BOXES AND VALVE BOXES:**

|  |  |  |
| --- | --- | --- |
| (11-15-22) | 858 | SP8 R98R |

Revise the *2018* *Standard Specifications* as follows:

**Page 8-38, Article 858-4 MEASUREMENT AND PAYMENT,** lines 10-11, delete and replace the fifth paragraph with the following:

Where any catch basin, drop inlet, manhole, meter box or valve box is adjusted more than once because of milling operations, each adjustment will be measured and paid.