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This project lies just underneath approach, departure, and circling airspace for the [Airport]____________________.  Obstructions to airspace are a serious consideration.  The Contractor is notified that certain FAA provisions apply.

The Contractor shall not use any means or measure which will cause a temporary obstruction (such as cranes and soil or equipment stockpiles) whereby any component of the obstruction is higher than [Number of Feet Above Mean Sea Level]____________________ feet above mean sea level.  Before extending/raising any crane for the first time at each usage site, the Contractor shall verify crane setup (with regard to elevations) with the Engineer and obtain approval to extend/raise the trestle or boom.

At all times while on site, all cranes,  equipment, or temporary stockpiles taller than 50 feet in height shall be outfitted with an operational FAA-approved obstruction warning light system that engages automatically (photosensitive switch) each night.  The Contractor shall submit proof that the system is FAA-approved, that power systems are operational, and that two replacement bulbs are on site prior to the equipment being allowed to be used or extend vertically on site.  Reference:  FAA Advisory Circular 150/5345-43.

Unless otherwise approved in writing by NCDOT, the Contractor shall not locate any component of a borrow pit within 10,000 feet of the end of any runway at [Airport]____________________.  The Contractor shall be responsible for meeting all conditions required by the FAA for the temporary works and equipment.

All costs incurred by the Contractor in complying with all FAA and [Airport]____________________ requirements shall be included in the prices bid for the various pay items and no additional payment will be made.

