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Lump sum grading shall be performed in accordance with Section 226 Comprehensive Grading of the Standard Specifications except as follows:

Delete all references to [Fill-in from choices below]_________________________________.

Section 200, Clearing and Grubbing

Section 225, Roadway Excavation

Section 230, Borrow Excavation

Section 250, Removal of Existing Asphalt Pavement

Section 250, Removal of Existing Concrete Pavement

Section 250, Breaking of Existing Asphalt Pavement

Section 250, Breaking of Existing Concrete Pavement

Section 500, Fine Grading

Section 560, Shoulder Borrow


INSTRUCTIONS

This provision should be used only when Item 0063 Lump Sum Grading is included in estimate.  In addition, one or more of the following Items will also be included in estimate:

0001 - Clearing and Grubbing
0022 - Unclassified Excavation
0106 - Borrow Excavation
0156 - Removal of Existing Asphalt Pavement
0163 - Removal of Existing Concrete Pavement
0177 - Breaking of Existing Asphalt Pavement
0185 - Breaking of Existing Concrete Pavement
1011 - Fine Grading
1231 - Shoulder Borrow

If Item 0043 Lump Sum Grading is included, none of the above items will be in estimate.

