REMOVAL OF EXISTING SHOULDER:
	(4-15-08)
	SPI 2-07



In areas where the existing shoulder is to be converted to full depth paved shoulder, the Contractor shall remove all asphalt, earth material and aggregate necessary to place the proposed asphalt base course in accordance with the typical section and as directed by the Engineer.

No separate payment shall be made for the removal of existing shoulder as the cost of this work shall be included in the unit price bid per ton for Asphalt Concrete Base Course, Type B25.0B.

