PIPE ALTERNATES (with elbows):
	   (5-17-12)(Rev. 1-16-24)
	SPI 3-04



Description

The Contractor may substitute Aluminized Corrugated Steel Pipe, Type IR, Aluminized Corrugated Steel Pipe Elbows, Type IR or HDPE Pipe, Type S or Type D up to 48 inches in diameter in lieu of concrete pipe in accordance with the following requirements.

Material

	Item
	Section

	HDPE Pipe, Type S or D
	1032-7(A)

	HDPE Pipe Elbow and Tees
	1032-7(B)

	Corrugated Aluminum Alloy Pipe Culvert
	1032-2(A)

	Corrugated Aluminum Alloy Pipe Tees and Elbows
	1032-2(B)



Aluminized Corrugated Steel Pipe will not be permitted in counties listed in Article 310-2 of the Standard Specifications.

Construction Methods

Corrugated Aluminum Alloy Pipe Culverts, Corrugated Aluminum Alloy Pipe Tees and Elbows, and HDPE Pipe Culverts shall be installed in accordance with the requirements of Section 300 of the Standard Specifications for Method A, except that the minimum cover shall be at least 12 inches.  Corrugated Aluminum Alloy Pipe Culvert and HDPE Pipe Culvert will not be permitted for use under travelways, including curb and gutter.  

Measurement and Payment

___ "C.A.A. Pipe Culvert, ____ " Thick to be paid for will be the actual number of linear feet installed and accepted.  Measurement will be in accordance with Section 310-6 of the Standard Specifications.

___ " C.A.A. Pipe Elbows, ____ " Thick and ___ " x ___ " x ___" C.A.A. Pipe Tees will be measured and paid for in units of each for the actual number incorporated into the completed and accepted work.  Measurement will be made in accordance with Section 310-6 of the Standard Specifications.

___" HDPE Pipe Culvert to be paid for will be the actual number of linear feet installed and accepted.  Measurement will be in accordance with Section 310-6 of the Standard Specifications.

___ " HDPE Pipe Elbows, ____ " Thick and ___ " x ___ " x ___" HDPE Pipe Tees will be measured and paid for in units of each for the actual number incorporated into the completed and accepted work.  Measurement will be made in accordance with Section 310-6 of the Standard Specifications.

Payment will be made under:

	Pay Item
	Pay Unit

	___ " HDPE Pipe Elbows, ____ "
	Each

	___ " x ___ " x ___" HDPE Pipe Tees
	Each



