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Description

Furnish and install polymer drain lines and grates and frames in accordance with the contract documents.

Materials

The precast concrete drain line shall be manufactured using polyester polymer concrete.  The polymer concrete shall have a minimum compressive strength of 17,250 psi (118.9MPa).

The concrete encasement adjacent and beneath the channel shall be Class B in accordance with the Standard Specifications.

The grates and frames shall meet the requirements of AASHTO M 306 Ductile Iron with 50,000 pound proof load rating.

Construction Methods

The precast unit shall be installed in accordance with the details in the plans.

Measurement and Payment

Polymer Drain Line will be measured and paid for as the actual number of linear feet incorporated in the completed and accepted work.  Measurement will be made along the surface of the drain line.  No separate payment will be made for the grates and frames as the cost shall be included in the unit bid price for the drain line.

Payment will be made under:

	Pay Item
	Pay Unit

	Polymer Drain Line
	Linear Foot 



