INSPECTION VESSEL:
	(4-16-16)
	SPI 4-06



Description

Furnish a new vessel in accordance with this special provision for inspection of this project by NCDOT personnel. 

Minimum Specifications

Provide a fiberglass hull boat with an outboard engine and galvanized steel trailer having the following minimum specifications and equipment:

	(1) Centerline length (20’-10”)

	(2) Beam (93 in)

	(3) Outboard engine shall be four stroke & a minimum of 140 horse power and shall be equipped with power trim and tilt, and overheat alarm.  The brand of engine shall be such that parts and service shall be readily available in eastern North Carolina.

	(4) On-board fuel capacity (19 gallons)

	(5) Stainless steel propeller of diameter and pitch to operate the vessel in accordance with the manufacturer’s recommendations

	(6) Self-bailing

	(7) Non-skid floor

	(8) Non-snag bow light and removable stern light

	(9) Heavy duty rub rail

	(10) Heavy duty battery

	(11) Bilge inspection plate

	(12) Large center console with wrap around windshield

	(13) Hydraulic steering system 
(14) Fuel/water separator

	(15) Watertight fiberglass box seat (front of center console) with cushion back and removable self-supporting cushion seat.

	(16) Automatic bilge pump

	(17) Tachometer

	(18) Spray hood and Bimini top

	(19) Danforth-type anchor of sufficient size with 200 ft of anchor line

	(20) Bow and stern line

	(21) Signal kit

	(22) Seven (7) vest-type life preservers

	(23) Throw ring buoy with 100 ft of line

	(24) Fire extinguisher

	(25) Any other equipment that may be required by the U.S. Coast Guard for the safe operation of the vessel

	(26) VHF console mounted marine grade waterproof radio, must be able to connect with U. S. Coast Guard channels

	(27) All lines shall be nylon and of sufficient size for the intended use

	(28) Whistle

	(29) Heavy duty, tandem axle trailer.  The trailer shall be aluminum, all components and hardware shall be non-corrosive, including the wheels and axle and shall be equipped with lights, winch, a mounted spare wheel and tire and appropriate ball to fit trailer. 



The boat, engine and trailer shall be compatible, new, current models and meet all applicable U.S. Coast Guard regulations.  The Contractor shall submit to the Engineer the manufacturer’s specifications of the proposed boat, engine and trailer for approval.

Ownership and Delivery

Deliver the vessel to the Engineer to LOCATION.  At this time the ownership shall be transferred to the Department.  The vessel shall be delivered prior to any water work beginning. 

Measurement and Payment

Inspection Vessel will be paid at the contract lump sum price.  for Inspection Vessel.  Payment shall be full compensation for furnishing the boat, engine, and trailer, and accessories as listed in this special provision. 

Payment will be made under:

	Pay Item
	Pay Unit

	Inspection Vessel
	Lump Sum




