
MEDIAN CROSSOVER:
	   (5-18-04)(Rev. 1-16-24)
	SPI  05 - 06



Description

The Contractor shall construct a median crossover at the location indicated on the plans, in accordance with the detail in the plans and as directed by the Engineer.

Materials

The sand shall meet the requirements of Sub Article 1012-1(C) of the Standard Specifications.

The #57 stone shall meet the requirements of Section 1005 of the Standard Specifications.

The paving blocks shall match as closely as possible the dimensions and pattern shown in the detail in the plans.

Fill the cores of the paving blocks with topsoil with a P.I. greater than 6 and less than 25 and with a pH ranging from 5.5 to 6.8.

Measurement and Payment

The quantity of median crossover to be paid for will be the actual number of square yards of median crossover which have been incorporated into the completed and accepted work.

The quantity of median crossover, measured as provided above, will be paid for at the contract unit price per square yard for Median Crossover.  Such price and payment will be full compensation for all material, labor and incidentals to complete the work.  No separate measurement and payment will be made for filling the paving block cores with topsoil and seeding as such work shall be incidental to the work of Median Crossover.

Payment will be made under:

	Pay Item
	Pay Unit

	Median Crossover
	Square Yard




