SHOULDER RECONSTRUCTION PER SHOULDER MILE:
	(1-18-00) (Rev 8-21-12)
	SPI 05-07



Description

This work consists of reconstructing each shoulder (including median shoulders as applicable) in accordance with Roadway Standard Nos. 560.01 and 560.02 except that the rate of slope and width will be as shown on typical section, or to the existing shoulder point, whichever is nearer, as long as the desired typical is achieved.  This work shall be performed immediately after the resurfacing operations are complete as directed by the Engineer.

Materials

The Contractor shall use Aggregate Shoulder Borrow (ASB) which meets the following gradation on all maps unless otherwise directed by the Engineer.

	Sieve
	Percent Passing

	1 1/2”
	100

	1/2”
	55 – 95

	#4
	35 – 74



Construction Methods

Obtain material from within the project limits or approved borrow source.  Material shall be compacted to the satisfaction of the Engineer.

Any excess material generated by the shoulder reconstruction shall be disposed of by the Contractor in an approved disposal site.

Measurement and Payment

Shoulder Reconstruction will be measured and paid for as the actual number of miles of shoulders that have been reconstructed.  Measurement will be made along the surface of each shoulder to the nearest 0.01 of a mile.  Such price will include disposing of any excess material in an approved disposal site for all labor, tools, equipment, and incidentals necessary to complete the work.

Incidental Stone Base will be measured and paid for as provided in Article 545-6 of the Standard Specifications.  If ASB is used for Incidental Stone Base, payment will be made for Aggregate Shoulder Borrow as referenced above.

Payment will be made under:

	Pay Item 
	Pay Unit

	Shoulder Reconstruction
	Shoulder Mile

	Aggregate Shoulder Borrow
	Ton



