CONCRETE STEPS:
	(11-18-08)
	SPI 8-03



Description

Construct reinforced concrete steps in accordance with the contract documents.  

Materials

Refer to Division 10 of the Standard Specifications:

	Item
	Section

	Portland Cement Concrete, Class B
	1000

	Curing Agents
	1026

	Steel Bar Reinforcement
	1070-2



Construction Methods

Construct concrete in accordance with Section 825 of the Standard Specifications, except as otherwise provided herein.  Furnish and place reinforcement, as shown on the plans, in accordance with Section 425 of the Standard Specifications.  Give formed surfaces of the concrete a rubbed finish. Give unformed surfaces a float finish.  Compact backfill to a degree comparable to the adjacent undisturbed material.

Measurement and Payment

Concrete Steps will be measured and paid for in cubic yards computed from the dimensions shown on the plans or established by the Engineer that has been incorporated into the completed and accepted steps.  Work includes but is not limited to excavation and backfilling, furnishing and placing concrete, reinforcing steel, and all labor, tools, materials, equipment and incidentals necessary to complete the work.

Payment will be made under:

	Pay Item
	Pay Unit

	Concrete Steps
	Cubic Yard



