CONCRETE STEPS (with handrail):
	(Rev 11-7-08)
	SPI 8-04



Description

Construct reinforced concrete steps with handrails in accordance with the plans and contract documents.

Materials

Refer to Division 10.

	Item
	Section

	Portland cement concrete, Class B
	1000

	Curing agents
	1026

	Steel bar reinforcement
	1070-2

	Galvanizing
	1076

	Steel Pipe Rail
	ASTM A53 (schedule 40)Plain End Galvanized Pipe



Construction Methods

Construct concrete in accordance with Section 825, except as otherwise provided herein.  Furnish and place reinforcement, as shown on the plans, in accordance with Section 425.  Give formed surfaces of the concrete a rubbed finish. Give unformed surfaces a float finish.  Compact backfill to a degree comparable to the adjacent undisturbed material.

Measurement and Payment

Concrete Steps will be measured and paid for in cubic yards computed from the dimensions shown on the plans or established by the Engineer that has been incorporated into the completed and accepted steps.  Work includes but is not limited to excavation and backfilling, furnishing and placing concrete, reinforcing steel, steel pipe rail, grout and all labor, tools, materials, equipment and incidentals necessary to complete the work.

Handrail on Steps will be measured and paid in linear feet along the top of the rail to the nearest 0.1 foot.  Such price shall include furnishing and installing handrails, grouting, painting, and all labor, tools, equipment and incidentals necessary to complete the work.

Payment will be made under:

	Pay Item
	Pay Unit

	Concrete Steps
	Cubic Yard

	Handrail on Steps
	Linear Foot



	
