

TEMPORARY TRUCK ESCAPE RAMP:
	   (7-1-95)
	SPI 8-06



Description

The work covered by this provision consists of constructing a temporary truck escape and concrete dead man in accordance with the details in the plans and as directed by the Engineer the Contractor shall remove and dispose of the temporary truck escape ramp and concrete dead man and all related items.  

Materials

The aggregate shall meet the requirements of Section 1005 of the Standard Specification.

The concrete dead man shall be constructed of Class A concrete meeting the requirements of Section 1000 of the Standard Specifications.  The reinforcing steel shall meet the requirements of Section 1070 of the Standard Specifications.

Measurement and Payment

No measurement will be made for constructing the Temporary Truck Escape Ramp.

The quantity of concrete dead men to be paid for will be the actual number of Concrete Dead Man which have been constructed and accepted.

Payment for constructing the temporary truck escape ramp will be made at the contract lump sum price for Temporary Truck Escape Ramp.

The quantity of concrete dead men, measured as provided for above, will be paid for at the contract unit price per each for Concrete Dead Man.

The above prices and payments will be full compensation for all work covered by this provision including but not limited to furnishing and placing the aggregate, concrete, reinforcing steel; labor, equipment, removing and disposing of the escape ramp at the proper time, and all incidentals necessary to complete the work.

Payment will be made under:

	Pay Item
	Pay Unit

	Temporary Truck Escape Ramp
	Lump Sum

	Concrete Dead Man
	Each



						  
