DRAINAGE STRUCTURE REPAIR:
	(11-17-09)
	SPI 8-20



Description

The Contractor shall remove grates and frames from existing drainage structures and shall replace existing deteriorated brick layers of the drainage structures with new brick layers.  Removal of existing brick layers shall be as directed by the Engineer.  Placement of new brick shall be in accordance with Section 840 of the Standard Specifications.

Measurement and Payment

Drainage Structure Repair will be measured and paid for in units of linear feet for the actual height of new brick layers in the drainage structure that have been completed and accepted.  Such price and payment includes but is not limited to, providing all materials, removing and disposing of existing brick layers, placing all brick, excavating and backfilling, removing and placing back of the existing grates and frames, and all incidentals necessary to complete the work.  

Payment will be made under:

	Pay Item
	Pay Unit

	Drainage Structure Repair
	Linear Foot



