CURB CUTS AT SIDEWALK:
	(11-17-09)
	SPI 8-22



Description

This work consists of constructing a curb cut with flume and furnishing and installing a traffic bearing steel plate for curb cut.

Materials

Submit catalog cuts and shop drawings for the traffic bearing steel plate for approval.  The submittal shall show the material description, brand name, manufacturer name, size and rating.  Do not deliver materials that have not been approved to the project.  

Construction Methods

Construct curb cuts with flume and Traffic Bearing 30" Steel Plate for Curb Cuts in accordance with the detail in the plans at locations indicated in the plans.  

Measurement and Payment

Curb Cut with Flume and Traffic Bearing 30" Steel Plate for Curb Cut will be measured and paid in units of each that have been incorporated into the completed and accepted work.

Payment will be made under:

	Pay Item
	Pay Unit

	Curb Cut with Flume
	Each

	Traffic Bearing 30" Steel Plate for Curb Cut
	Each



