FRAME WITH GRATE (Driveway Drop Inlet):
	   (3-21-00)(Rev. 1-16-24)
	SPI 8-35



Description

Provide grates for driveway drop inlets that are fabricated steel or cast iron.  Provide grates that are of a design and weight that is recommended by the manufacturer as being adequate for HS‑20 loadings.  Furnish a manufacturer's certification stating that the grates and frame furnished on the project have been designed and manufactured to be adequate for an HS-20 loading.  Provide grates with a minimum clear waterway opening of 50 in2 per 1'-0" length of grate.

If the frame and grate is made from fabricated steel, the requirements of Article 1074-9 of the Standard Specifications will be applicable. If the grate and frame is made from iron castings, the requirements of Article 1074-7 of the Standard Specifications will be applicable.

Measurement and Payment

Frame with Grate, Driveway Drop Inlet will be measured and paid for as the actual number of linear feet that have been incorporated into the completed and accepted work.  Such price and payment will be full compensation for furnishing the grates and frame, and all labor and incidentals necessary to complete the work.

Payment will be made under:

	Pay Item
	Pay Unit

	Frame with Grate, Driveway Drop Inlet
	Linear Foot



