
ALUMINUM PICKET FENCE:
	(3-5-14)
	
	SPI 8-41



Description

Construct aluminum picket fence that complies with the plans and this provision.

Materials

See detail in the plans for material requirements and use powder-coated black components.

Construction Methods

Construct the aluminum picket fence in accordance with the detail in the Plans.  Clear and grub fence site in accordance with Subarticle 866-3(A) in the Standard Specifications.

Set and maintain all posts in a vertical position.  Line posts may be hand set or set with a post driver.  Thoroughly tamp all backfilled material if hand set.  If power driven, remove and replace posts that are damaged by power driving.

Set posts in concrete anchors to maintain the position and alignment of the post when required in the plans or where dictated by soil conditions.  Forms are not required for the concrete.  Trowel the top of the concrete to a smooth finish and slope to drain away from the post.  The concrete anchors require at least a 3 day curing period before any load is placed on the post.

Drive the posts at least 3 feet into the ground.  Provide adequate protection to the post tops to prevent damage from the driving operations.  Repair damage to the powder coated paint.  Set posts in concrete anchors where soil conditions are such that the posts cannot be driven without deformation, or where soils are encountered that does not provide adequate in-ground stability.

Where rock or concrete pavement or slabs are encountered within the required depth where fence posts are to be erected, drill a hole in the rock or concrete of a diameter slightly larger than the largest dimension of the post in the rock or concrete and grout in the post.  The depth of post embedment shown in the plans will not be required and the post may be shortened as necessary, provided the post is embedded within the rock or concrete pavement or slab to a minimum depth of 12 inches.

Do not fabricate extra length posts by welding short sections of posts together.

Measurement and Payment

Aluminum Picket Fence will be measured and paid per linear foot of fence satisfactorily completed and accepted.  All posts used for the aluminum picket fence are included in the price of the aluminum picket fence and will not be paid separately. Such price and payment shall be full compensation for all labor, materials and incidentals to complete the work.

Payment will be made under:

	Pay Item
	Pay Unit

	Aluminum Picket Fence
	Linear Foot



