
ENERGY DISSIPATOR:
	(2-17-98)
	SPI 8-43



Description

Construct a concrete energy dissipator according to the details and in the locations shown on the plans.  Provide all excavation, backfill, labor and material to complete this item of work.  Structure may be cast-in-place or precast.

Material

Provide all material in accordance with Section 840-2 or Article 1077-3 of the Standard Specifications as applicable.  Use Class B concrete for cast-in-place or 28 MPa (4000 psi) for precast.

Construction Methods

Perform all work in accordance with Section 840 or Section 1077 of the Standard Specifications as applicable.

Measurement and Payment

Energy Dissipator will be measured and paid in units of each.  The quantity paid for will be the actual number completed and accepted.

Payment will be made under:

	Pay Item
	Pay Unit

	Energy Dissipator
	Each



