RIPRAP ENERGY DISSIPATOR BASIN:
	(10-14-09) (Rev. 2-7-14)
	SPI 8-44



Description

This work consists of the construction and maintenance of an armored outlet structure located at culvert outlets or ditch termini. 

Materials
Refer to Division 10 of the Standard Specifications.

	Item
	Section

	Class I Riprap 
	1042

	Geotextile for Drainage, Type 2
	1056



Construction Methods

Riprap energy dissipators shall be constructed in accordance with the detail shown in the plans or as directed by the Engineer.  From the outlet, invert of a culvert or bottom of a ditch excavation will drop to a specified depth.  Excavation will continue to widen through the dissipator.  Riprap shall be placed along the banks and bottom of the dissipator and along the apron.

Excavate ditch in accordance with Section 240 of the Standard Specifications.

The quantity of energy dissipator material may be affected by site conditions during construction of the project.  The quantity of materials may be increased, decreased, or eliminated at the direction of the Engineer.  Such variations in quantity will not be considered as alterations in the details of construction or a change in the character of the work.

Measurement and Payment

Energy Dissipator Basin will be paid on a lump sum basis.  Such price and payment will be full compensation for all work covered by this section, including, but not limited to, furnishing and placing stone, filter fabric, materials, labor, tools, equipment, and incidentals necessary to complete the work.

Payment will be made under:

	Pay Item
	Pay Unit

	Energy Dissipator Basin
	Lump Sum



