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The Contractor's attention is directed to Section 840 of the Standard Specifications.

Provide a Frame with Cover with the cover bolted to the frame.  Provide 2 – 5/8" stainless steel bolts for each frame with cover that meet the requirements of Article 1072-5 of the Standard Specifications.

