IMPACT ATTENUATOR UNITS, TYPE ___ (EXTENDED LIFE):
	(8-15-17)(Rev. 10-17-23)  
	SPI 8-47



Description

Furnish and install impact attenuator units and any components necessary to connect the impact attenuator units in accordance with the manufacturer’s requirement, the details in the plans and at locations shown in the plans.

Materials

Furnish impact attenuator units listed on the NCDOT APL under the category “Impact Attenuator, Life Cycle”.  Units shall not be modified by the manufacturer and installer once approved and on the NCDOT APL.

Prior to installation the Contractor shall submit to the Engineer certified working drawings and assembling instructions from the manufacturer for each impact attenuator unit in accordance with Article 105-2 of the Standard Specifications.

Construction Methods

Perform installation in accordance with the plans and details and assembling instructions furnished by the manufacturer.

Measurement and Payment

Impact Attenuator Unit, Type ___ (Extended Life) will be measured and paid for at the contract unit price per each completed and accepted by the Engineer.  Such prices and payment will be full compensation for all work covered by this provision including but not limited to furnishing, installing and all incidentals necessary to complete the work.

Payment will be made under:

	Pay Item
	Pay Unit

	Impact Attenuator Unit, Type ___ (Extended Life)
	Each



