
HIGH TENSION CABLE BARRIER SYSTEM WITH REPAIR ITEM:
	(2-19-09)(Rev. 8-17-21)
	SPI 08-49



Description

Furnish, install and repair MASH compliant rope/cable barrier system in accordance with the manufacturer’s recommendation and as directed by the Engineer.  On the plans it will be labeled as High Tension Cable Barrier.

Materials

Furnish cable barrier systems listed on the NCDOT APL.

The cable barrier system shall meet the following minimum specifications:

1) Have a 8 foot Maximum Deflection
2) Install a minimum distance of 8 feet from centerline of Median Ditch
3) Capable of withstanding additional vehicle impact into same area prior to repair
4) Socketed / Sleeved Foundation

Construction Methods

High Tension Cable Barrier installation shall be in accordance with the manufacturer’s recommendations.

Prior to installation the Contractor shall submit to the Engineer certified working drawings and assembling instructions from the manufacturer for the cable barrier system in accordance with Section 105-2 of the Standard Specifications.

Perform installation in accordance with the details in the plans, and details and assembling instructions furnished by the manufacturer.

Prior to acceptance, the Contractor shall submit a certification stating that the High Tension Cable Barrier meets the manufacturer’s specifications for materials and installation.

Repairs To Cable Barrier

Where vehicle accident damage has occurred to any portion of the cable barrier, the Contractor shall make satisfactory repairs within 72 hours after being notified by the Engineer. Satisfactory repairs will, in general, consist of straightening bent posts, reattaching cable, and retensioning the cable. However, in more severe instances, the Engineer may direct that new posts, anchors, and cable be installed. Each instance of cable barrier repair for accident damage performed as directed within a maximum 500 foot length will be counted.

Measurement and Payment

The quantity of High Tension Cable Barrier to be paid for will be the actual number of linear feet of cable barrier which has been satisfactorily completed and accepted exclusive of that length of cable barrier which is within the pay limits of cable anchors.  Measurement will be made from center to center of the outermost post in the length of cable barrier being measured.

The quantity of High Tension Cable Barrier Anchor to be paid for will be the actual number of units which have been completed and accepted.

The quantity of Repairs to Cable Barrier to be paid for will be the number of repairs for each instance of repair up to a length of 500 feet. 

The accepted quantities of High Tension Cable Barrier measured as provided above, will be paid for at the contract unit price per linear feet, complete-in-place, including installing all posts, anchorages, wire rope / cable, fittings, reflectors, excavation, concrete, backfill, compaction, shoulder build-up, and all labor, tools, equipment and incidentals necessary to complete the work.

The accepted quantities of High Tension Cable Barrier Anchor, measured as provided above, will be paid for at the contract unit price per each, complete in place, including all fittings, hardware, deflection posts, excavation, forming, backfill, compaction, concrete, safety check rope, end anchors, and all other labor, tools, equipment and incidentals necessary to complete the work.

Payment at the contract unit price per each for Repairs to Cable Barrier will be considered full compensation for all labor, tools, equipment, materials and incidentals to perform satisfactory repairs for each instance of repair up to a length of 500 feet. 

Any tension metering device required by the manufacturer for proper installation and/or repair of the cable barrier shall become the property of the Department after final acceptance of the project.

Payment will be made under:

	Pay Item
	Pay Unit

	High Tension Cable Barrier
	Linear Feet

	High Tension Cable Barrier Anchor
	Each

	Repairs to Cable Barrier
	Each



