REMOVE AND REPLACE ___" CONCRETE PAVED DITCH:
	(10-20-26)
	SPI 8-62



Description

Remove, dispose and replace damaged existing concrete paved ditches within the limits shown in the plans or as directed by the Engineer.  All work for this item shall be in accordance with Section 850 of the Standard Specifications and as shown on Roadway Standard Drawings No. 850.01 except that the concrete paved ditch width shall match existing.

[bookmark: _Hlk201740431]Materials

Use concrete paved ditch materials meeting the requirements of Article 850-2 of the Standard Specifications.

Construction Methods

Remove and replace concrete paved ditch at locations indicated in the plans or as directed by the Engineer.  After removing, grade to drain in accordance with the plans and as directed by the Engineer.

Dispose of materials and debris in an approved disposal site in accordance with Section 802 of the Standard Specifications, federal, state and local regulations. Disposal of existing ditch materials shall be incidental to the work.

Construct concrete paved ditch in accordance with Article 850-1 and 850-3 of the Standard Specifications.

Measurement and Payment

Remove and Replace ___" Concrete Paved Ditch  will be measured and paid for in square yards that is completed and accepted.  Longitudinal measurements will be made along the surface of the pavement at the centerline of the ditch and transverse measurements will be made along the surface of the pavement at right angles to the centerline. No measurement will be made of curtain walls at the beginning or ends of the paved ditches.  Such price and payment will be full compensation for removal and disposal of existing materials, excavating, backfilling, grading, furnishing, forming, placing all concrete, finishing, constructing curtain walls, constructing and sealing joints, and all incidentals necessary to complete the work.

Payment will be made under:

	Pay Item
	Pay Unit

	Remove and Replace ___" Concrete Paved Ditch
	Square Yard



