CHAIN LINK FENCE WITH REDWOOD PICKETS:
	(7-1-95)
	SPI 8-75



Description

Except for the size of the mesh, construct the chain link fence with redwood pickets in accordance with the plans, Section 866 of the Standard Specifications, and the following requirements. 

Construction Methods

Insert 2 1/2" x 3/8" red stained redwood pickets into the fabric vertically and permanently secure in place with rust resistant staples.  Provide fabric mesh of an appropriate size to accept the redwood pickets. 

Measurement and Payment

The quantities of Chain Link Fence, __" Fabric with Redwood Pickets and of gates to be paid for shall be measured for payment as provided in Section 866 of the Standard Specifications. 

The quantity of Chain Link Fence, ___" Fabric with Redwood Pickets, measured as provided above, will be paid for at the contract unit price per linear foot for Chain Link Fence, ___" Fabric with Redwood Pickets. 

The above prices and payments will be full compensation for all materials, labor, and incidentals necessary to complete the work.

Payment will be made under:

	Pay Item
	Pay Unit

	Chain Link Fence, __" Fabric with Redwood Pickets
	Linear Foot



