ERECTING FENCE ON RETAINING WALL:
	(4-15-08)
	SPI 8-78


 
Description

Erect the proposed fencing on the retaining wall at locations shown in the plans.  Install sleeves in the retaining wall in accordance with details in the retaining wall plans.  After the posts have been set in the sleeves, fill the space around the posts with molten lead, sulfur, or other material approved by the Engineer. 

Measurement and Payment

No direct payment will be made for erecting the fence on the retaining wall as required above as such work will be considered incidental to the work being paid for at the contract unit prices for the various fencing items involved.

