GROUT FOR HDPE PIPE LINER:
	   (7-19-12)(Rev. 1-16-24)
	SPI 10-02



Description

Furnish and install grout between the HDPE Pipe and the existing CS Pipe as shown in the plans.

Materials

Use a grout which has a minimum compressive strength of 3,000 psi at three days and which meets the applicable requirements of Section 1003 of the Standard Specifications.

Construction Methods

Place the grout by pumping, pouring or other approved method.

Measurement and Payment

Grout will be measured and paid for as the number of cubic yards that is incorporated around the HDPE pipe liner.  The number of cubic yards of grout is computed from dimensions in the plans.

Payment will be made under:

	Pay Item
	Pay Unit

	Grout
	Cubic Yard



