PVC PIPE:
	(3-20-07)
	SPI 10-06



Description

Furnish and install PVC pipe in accordance with the Standard Specifications, plans or as otherwise directed by the Engineer.

Materials

Refer to Division 10 of the Standard Specifications:

	Item
	Section

	PVC Pipe 
	1034



Use pipe meeting the requirements for Gravity Flow Sewer Pipe.

Construction Methods

Install PVC pipe in accordance with Section 300 of the Standard Specifications and as directed by the Engineer.

Measurement and Payment

____" PVC Pipe will be measured and paid as the actual number of linear feet of pipe that has been incorporated into the completed and accepted work. Measurement of pipe will be made by counting the number of joints used and multiplying by the length of the joint to obtain the number of linear feet of pipe installed and accepted. Measurements of partial joints will be made along the longest length of the partial joint to the nearest 0.1 feet. Select bedding and backfill material will be included in the cost of the installed pipe. Such price and payment will be full compensation for all materials, labor, equipment, and other incidentals necessary to complete the work.

Pipe End Sections, Tees, Elbows, Couplers and Eccentric Reducers will be measured and paid in units of each that have been incorporated into the completed and accepted work in accordance with this special provision or Article 310-6 of the Standard Specifications.

Payment will be made under:

	Pay Item
	Pay Unit

	____" PVC Pipe
	Linear Foot

	____" PVC Pipe Elbows, __" Thick
	Each

	__" x __" x__" PVC Pipe Tees, __" Thick
	Each



