DEPARTMENT FURNISHED PORTABLE CONCRETE BARRIER:
	  (7-8-15)
	SPI 11-03



Description

Obtain, install, secure, maintain, refurbish, remove, and return Department Furnished Portable Concrete Barrier in accordance with the plans, contract and specifications. 

Materials

The Department will provide Portable Concrete Barrier in accordance with 1170-2 of the Standard Specifications.  Obtain the barrier from the stockpile on I-40 at Exit 15.

Provide connecting pins for the Department furnished Portable Concrete Barrier of the size and type required for the Department furnished barrier.

Construction Methods

Obtain and return Department Furnished Portable Concrete Barrier in accordance with 1170-3 of the Standard Specifications at the location(s) specified in the plans.

Engineer will inspect Portable Concrete Barrier prior to the Contractor accepting responsibility of the barrier.  Contractor is fully responsible for any damage or theft after acceptance.

Transport Portable Concrete Barrier to the project and provide necessary storage area for the barrier at no cost to the Department.

Refurbish and maintain barrier in good operational condition.  Return barrier in good operational condition including all manuals, maintenance records, special tools, hardware, etc.

Measurement and Payment

Refer to Article 1170-4 of the Standard Specifications.

Payment will be made under:

	Pay Item
	Pay Unit

	Department Furnished Portable Concrete Barrier
	Linear Foot




