DECORATIVE CROSSWALK PAVEMENT MARKING:
	   (1-23-20)(4-16-24)
	SPI 12-03



Description

Provide decorative crosswalk pavement marking in accordance with Sections 1087 and 1205 of the Standard Specifications, the plans and the contract.  

Materials

Refer to Article 1205-2 of the Standard Specifications. 
 
Construction Methods
 
The surface of the product shall meet a minimum FN40R value SN 37 in accordance with ASTM E-274, Skid Resistance of Paved Surfaces.
 
The crosswalk is to be marked per MUTCD standards with parallel transverse lines. The lines must be applied with an approved pavement marking system per the Standard Specifications and shall be retroreflective.    
 
In addition to this special provision, the material and application shall comply with the TEPPL (Traffic Engineering Policies, Practices, and Legal Authority) topic C54- Decorative Crosswalks Standard Practice.   This practice can be found at https://connect.ncdot.gov/resources/safety/Teppl/Pages/Teppl-Topic.aspx?Topic_List=C54

Measurement and Payment

[bookmark: _Hlk160632048]Decorative Crosswalk Pavement Marking will be measured and paid as the actual number of square feet of decorative crosswalk pavement markings satisfactorily placed and accepted by the Engineer.  Such price and payment will be considered full compensation for all labor, materials, equipment and incidentals necessary to satisfactorily complete the work.

Payment will be made under:

	Pay Item
	Pay Unit

	Decorative Crosswalk Pavement Marking
	Square Foot
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