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Description

Provide profiled pavement marking lines in accordance with Sections 1087 and 1205 of the Standard Specifications, the details, the plans and the contract.  

Materials

Refer to Article 1205-2 of the Standard Specifications. 

The Contractor shall be certified to place the material by the manufacturer of that material.  At least one member of each crew working on this project shall have completed this training.  The Contractor shall furnish the Engineer written confirmation of this training from the material manufacturer prior to the beginning of work.  A manufacturer technical representative shall be onsite during the entire installation of the product. 

The profiled pavement marking lines shall have enough bond strength to resist the effect of snow removal equipment.

Construction Methods

Install in accordance with the manufacturer's recommendations. 

Hand liner type equipment shall not be allowed for installation.

The noise produced by driving a vehicle on the markings at the posted speed limit shall be at least 80 dBA as measured by any approved noise meter.

Measurement and Payment

Thermoplastic Profiled Pavement Marking Lines, ___" will be measured and paid as the actual number of linear feet of thermoplastic profiled pavement marking lines satisfactorily placed and accepted by the Engineer.  The quantity of lines will be the summation of the linear feet of lines measured end-to-end of the line.  Such price and payment will be considered full compensation for all labor, materials, equipment and incidentals necessary to satisfactorily complete the work.

	Pay Item
	Pay Unit

	Thermoplastic Profiled Pavement Marking Lines, ___"
	Linear Foot



