RESIDENTIAL SEEDING - LAWN TYPE APPEARANCE:
	   (7-20-10)
	SPI 16-01



All areas adjacent to lawns must be hand finished as directed to give a lawn type appearance.  Remove all trash, debris, and stones 3/4 inch and larger in diameter or other obstructions that could interfere with providing a smooth lawn type appearance.  These areas shall be reseeded to match their original vegetative conditions, unless directed otherwise by the Engineer.

Residential Seeding will be measured and paid in acres, measured along the surface of the ground over which residential seeding has been placed as directed and accepted by the Engineer.

Payment will be made under:

	Pay Item
	Pay Unit

	Residential Seeding
	Acre



