DRY DETENTION BASIN:
	   (6-21-09)
	SPI 16-03



Description

This work consists of the construction and maintenance of a basin at locations designated on the plans. Provides temporary storage of storm runoff and attenuates peak flows. Includes placement of riser/drawdown structures.

The size of the detention basin and drawdown structure may be effected by site conditions during construction of the project.  The quantity of materials may be increased, decreased, or eliminated entirely at the direction of the Engineer. Such variations in quantity will not be considered as alterations in the details of construction or a change in the character of the work.

Materials

Refer to Division 2, 8 and 10 of Standard Specifications.

	Item
	Section

	Minor Drainage Structure (Drawdown)
	840

	Drainage Ditch Excavation
	240

	PVC Pipe
	1034



Construction Methods

Dry detention basin is to be excavated and drawdown structure constructed as specified in the plans or as directed.

Measurement and Payment

Masonry Drainage Structure will be measured and paid for in accordance with Article 840-4 of the Standard Specifications.

Drainage Ditch Excavation will be measured and paid for in accordance with Article 240-4 of the Standard Specifications.

Such price and payment will be full compensation for all work covered by this section, including, but not limited to furnishing all materials, labor, PVC pipe, equipment, and incidentals necessary to construct the rock cross vanes.

