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Description

Furnish and install PVC conduit in accordance with Section 1715 of the Standard Specifications, the plans, or as otherwise directed by the Engineer.

Materials

Conduit shall meet the requirement of Article 1091-3 nonmetallic conduit.

Measurement and Payment

The quantity of conduit to be paid for will be the actual number of linear feet of conduit, which has been completed and accepted by the Engineer.

The quantity of PVC conduit measured as above will be paid for at the contract unit price per linear feet for ____" PVC Conduit.

Payment will be made under:

	Pay Item
	Pay Unit

	____" PVC Conduit
	Linear Foot



