**CLEARING AND GRUBBING - METHOD II:**

|  |  |  |
| --- | --- | --- |
| (9-17-02) (Rev. 3-19-24) | 200 | SP2 R02A |

Perform clearing on this project to the limits established by Method - II shown on Standard Drawing No. 200.02 of the *Roadway Standard Drawings*. Conventional clearing methods may be used except where permit drawings or conditions have been included in the proposal which require certain areas to be cleared by hand methods.