**CORRUGATED ALUMINUM ALLOY PIPE ARCH CULVERT:**

|  |  |  |
| --- | --- | --- |
| (9-17-24) | 310 | SP3 R36 |

Revise the *Standard Specifications* as follows:

**Page 3-7, Article 310-6, MEASUREMENT AND PAYMENT,** **lines 16,** delete “\_\_" C.A.A. Pipe Arch Culvert, \_\_" Thick” and replace with “\_\_" x \_\_" C.A.A. Pipe Arch Culvert, \_\_" Thick”.

**Page 3-7, Article 310-6, MEASUREMENT AND PAYMENT,** **lines 16,** delete “\_\_" x \_\_" x\_\_" C.A.A. Pipe Arch Tees, \_\_" Thick” and replace with “\_\_" x \_\_" x\_\_" x\_\_" C.A.A. Pipe Arch Tees, \_\_" Thick”.

**Page 3-7, Article 310-6, MEASUREMENT AND PAYMENT,** **lines 16,** delete \_\_" C.A.A. Pipe Arch Elbows, \_\_" Thick” and replace with “\_\_" x\_\_" C.A.A. Pipe Arch Elbows, \_\_" Thick”.