## MILLED RUMBLE STRIPS ON ASPHALT CONCRETE SHOULDERS:

|  |  |  |
| --- | --- | --- |
| (11-19-24)(Rev. 6-17-25) | 665 | SP6 R56 |

Revise the *Standard Specifications* as follows:

**Page 6-53, Article 665-3 CONSTRUCTION METHODS**, lines 20-21, delete and replace the first sentence of the second paragraph with the following:

Provide rumble strips that have finished dimensions of 7 inches ± 1/2 inch wide in the direction of travel and the length measured perpendicular to the direction of travel as specified in the contract.

**Page 6-53, Article 665-4 MEASUREMENT AND PAYMENT,** lines 30-33, delete and replace with the following:

*Milled Rumble Strips (Asphalt Concrete), \_\_\_*" will be measured and paid at the contract unit price per linear foot for the actual number of linear feet, measured longitudinally along the surface of each shoulder and/or edgeline, where rumble strips have been constructed.

Payment will be made under:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| Milled Rumble Strips (Asphalt Concrete), \_\_\_" | Linear Foot |