**CENTERLINE MILLED RUMBLE STRIPS ON ASPHALT CONCRETE:**

|  |  |
| --- | --- |
|  (4-18-23)(Rev. 11-19-24) | SP6 R57 |

**Description**

Construct centerline milled rumble strips on asphalt concrete in accordance with the plans, Section 665 of the *Standard Specifications* and as directed by the Engineer.

**Construction Method**

Construct centerline milled rumble strips in accordance with the applicable requirements of Section 665 of the *Standard Specifications* and as directed by the Engineer.

**Measurement and Payment**

*Centerline Milled Rumble Strips (Asphalt Concrete),* \_\_\_" will be measured and paid at the contract unit price per linear foot for the actual number of linear feet of centerline, measured longitudinally along the surface of centerline, where rumble strips have been constructed.

Payment will be made under:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| Centerline Milled Rumble Strips (Asphalt Concrete), \_\_\_" | Linear Foot |