**PAVING DRIVEWAYS AND MAILBOX TURNOUTS:**

|  |  |  |
| --- | --- | --- |
| (8-21-12) | 610 | SP6 R70BR |

Condition, prime, and surface all driveway and mailbox turnouts as directed by the Engineer. Place pavement on driveway and mailbox turnouts of the same material as used on the main line and in depths directed by the Engineer. Widen the pavement on curves as directed by the Engineer.