**REMOVE AND STOCKPILE EXISTING GUARDRAIL:**

|  |  |  |
| --- | --- | --- |
| (7-1-95)(Rev. 7-18-06) | 840, 859 | SP8 R55 |

**Description**

Carefully dismantle and remove existing guardrail and all components, concrete anchors included, at locations indicated in the plans and neatly stockpile it on the right of way, with the small parts stored in sturdy containers, for removal by State Forces. Dispose of the concrete anchors.

**Measurement and Payment**

*Remove and Stockpile Existing Guardrail* will be measured and paid as the actual number of linear feet of guardrail that has been satisfactorily removed and stockpiled. Measurement will be made from center to center of the outermost post in the length of guardrail being removed. Measurement will be made prior to removing the guardrail. Such price and payment will be full compensation for dismantling, removing, stockpiling, disposing of the concrete anchors, and all other incidentals necessary to complete the work.

Payment will be made under:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| Remove and Stockpile Existing Guardrail | Linear Foot |