**REMOVE IMPACT ATTENUATOR UNITS, TYPE \_\_\_\_\_:**

|  |  |  |
| --- | --- | --- |
| (3-18-25) |  | SP8 R74 |

**Description**

Dismantle, remove and dispose of existing impact attenuator unit at locations shown on the plans or as directed by the Engineer.

**Construction Methods**

Remove the existing impact attenuator unit in accordance with the plans without damaging adjoining structures or other appurtenances. Remove concrete or asphalt base in accordance with the plans without damaging adjoining pavement. Repair all damage at no cost to the Department as directed by the Engineer. All impact attenuator components and concrete or asphalt removed are the property of the Contractor. Do not remove traffic control if there are any exposed end of adjacent rail at the end of any day’s operation. Protect the exposed end of adjacent rail at the end of any day’s operations as directed by the Engineer. Backfill with compacted material to finish graded section or as directed by the Engineer.

**Measurement and Payment**

*Remove Impact Attenuator Units, Type \_\_\_\_\_* will be measured and paid in units of each. Such price and payment will be full compensation for the removal of the unit and base, disposal of unit and base, damage repair, backfilling and any incidentals necessary to complete the work.

Payment will be made under:

|  |  |
| --- | --- |
| **Pay Item** | **Pay Unit** |
| Remove Impact Attenuator Units, Type \_\_\_\_\_ | Each |