**PAVEMENT MARKING INSTALLATION REQUIREMENTS:**

|  |  |  |
| --- | --- | --- |
| (2-7-14) |  | SPD 02-700 |

All pavement markings shall be installed in accordance with Section 1205 of the *2018 Standard Specifications* and the following: The Contractor shall install two coats of paint pavement markings and beads on all portions of roadway that will be wintered-over.

**Measurement and Payment**

No payment will be made for installation or removal of pavement markings installed in order to over-winter a portion of the project.