## RAILROAD GRADE CROSSING:

|  |  |  |
| --- | --- | --- |
| (7-1-95) (Rev. 1-17-13) | 107-9 | SP1 G 17R |

Provide at least 2 weeks advance notice to the railroad's local Roadmaster or Track Supervisor when the use of slow-moving or stopped equipment is required over at-grade railroad crossings.